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AUTOMATIC CARTON ERECTOR

MODEL: CE-12
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Cleveland Equipment & Machinery Company
PREFACE   

Thank you for purchasing the auto carton sealer.
This manual will show you the basic structure, using method and points for attention to use this machine safely and correctly. Please read this manual carefully before operating the machine. Be sure that the manual is hand to the final users. This manual content change, without prior notice.
GPA carton sealer series use OPP tape to seal different kinds of cartons. The machine is operated and maintained easily with simple structure and high quality, for which it is widely used in various industries.

SAFETY INFORMATION
1. The operator should read the operating manual carefully before operating this machine.
2. The operator can not touch any driving parts before running this machine.
3. The maintenance personnel should read the operating manual carefully before maintaining this machine.
4. The power and gas must be closed when installing the tape and doing the daily maintenance.
5. Only the trained personnel can operate the machine.
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1 Specification
[image: ]
The carton erector is a Semi-auto carton sealing machine which can fold the bottom cover of carton and seal; it can be operated separately, economic and high-efficiency, which is an ideal packaging machine. The main parameters are listed as follows: 
Sealing speed：12ctns/min
Sealing width：150mm~400mm
Sealing height：100mm~400mm
Sealing lenght：250mm~450mm
Machine dimension：L2000 mm ×W1900 mm ×H1450 mm
Power supply：220v  1φ 200W
Air pressure：6kg/cm2
Applicable tape：W（48、60、72）mm×L1000y
Machine weight：450kg
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]2. Machine structure and adjustment instruction（P.1）：
[image: ]
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                   P.1

3. Operation flow
3.1 Operating instruction of the machine parts
1）Take out a formed carton
2）Turn the tape width adjusting hand wheel (clockwise, width of belt narrows, anticlockwise, width of belt widens), make the width the same with the carton width.( P.2)
[image: ]
P.2
3）Turn the adjusting hand wheel of the carton fetching system and make the acetabula surface is parallel with the strap surface when the acetabula is in the high-point.( P.3)
[image: ]
                        P.3
 4） Take out an unformed carton, put it onto the lower brim of the carton blocker, and then adjust the height and width of the carton storing trough, to make it the same as the unformed carton’s height and width.( P.4)
[image: ]
                      P.4
5) Adjust the cone-shaped adjuster，to make it align the carton folding line. (P.5)
[image: ]
                        P.5
[bookmark: OLE_LINK7][bookmark: OLE_LINK8]6）Turn the carton pushing adjust hand wheel to make the carton pushing pole, cone-shaped adjuster and the carton folding line in line. (P.6)
[image: ]
                         P.6
7）Adjust the acetabula to right position based the size of the carton . (P.7)

[image: ]
                         P.7
8）Finally put the unformed cartons into the carton storing trough, then lay down the pushing plate. (P.8)

[image: ]
                       P.8

3.2 Electrical control operation explaination
1）Make sure the machine is connected to the power supply and gas sources.
2）Start the NFB, start button by order, and make sure the emergence button is unpressed. (P.9)
[image: ]
                         P.9
3）After the machine is started, the LCD is shown as following. (P.10)
[image: ]
P.10
4）The main menu. (P.11)
Auto/ manual: to switch the auto interface or manual interface. Under the manual interface , press the “start” button to switch to the manual menu.
Counting：Showing the Quantity of  forming  cases. Push Zero can clear the record.
Erecting  Continually：Start this function when you run the machine automatically, then the machine erecting continually. 
Erect one case  ：Only form and seal one case.
Setting Out-Put  ：Showing the quantity of forming case. When you Push RST, the current Out-put becomes Zero. You can clear the Out-put to Zero in the High Level setting.

[image: ]
                         PIC 11      
5）Operate the machine manually according to the following picture 12:
      [image: ]
                        PIC12    
6）Set the Touch Scream 。
Basic setting, showing as Picture 13:
      [image: ]
                        PIC13
High Level Setting showing as Picture14:
[image: ]
PIC14
1、Click the first Icon to change the language.
 2、Click PLC, goes into IO/Input&output as the following picture15. 
[image: ]
PIC15
3、Click TIME to go and set time as the following Picture16 shows:
[image: ]
PIC16
4、Click BATCH OUT-PUT to set out-put as the following picture shows:
[image: ]
PIC17
8）Alarm rings to tell you information showing as the following picture:
[image: ]
PIC18
3.3Pneumatic  Parts  Instruction
1）Air-Pressure Drawing  showing as the following picture shows:
[image: ]PIC19
A、 It’s important to keep the Air pipes clean and do maintainance anytime.
B、 Please keep offering the air-pressure at 5～6kg/c㎡ to ensure the machine runs stably.  
C、 Cylinder Container: Keep the shaft clean, otherwise it causes air-leakage when the dust goes into the Piston.
D、 Maintainance on Air-Pipe: Remember to check if the air-pipe fluent and not blocked for folded. If it happens, please clear and make the air-pipe fluent for the air running.  
E、 Suckers: Keep the suckers clean and far away from the oil. It’s better to clean the Vacuum Contactor every week.
F、 The Three Points:
1、 Check if there’s enough oil in it, if not, add some in time. Please use the oil that is only for air-pressure, not too strong;
*Donot use the other oil instead, otherwise it causes air-flow-back, air-blocked and other problems;
2、Check the cup for water and drain away the water when it is too much inside；
3、Set the air-pressure to 5～6kg/c㎡.
H、When stop and do maitainance, please deflate the air by the Pressure release valve in case it does damage for operators. 
2）Electronic Drawing showing in the following Picture 20

PIC20
3）PLC  I/O  Showing As The Following Picture 21[image: ]                                 
                                   PIC21
3.4 Tape Head’s operating and Maintainance Showing As The Following Picture22:
1、Firstly, load the OPP tape on the tape holder showing as the following picture. Secondly, load the tape goes through the roller C and Roller B. Thirdly, it goes through Roller D. At last it goes out from Roller F after it comes out from the Tape Holder E as the picture shows. Pay attention that the sticky surface should be on the top. 
[image: ]        
                     PIC22
2、Adhesive Tape Loading Clue Drawing shows as the following picture23:
[image: ]
                                 PIC23
3、Adhesive Tape Position Adjusting Shows As The Following Picture24:
If the tape doesn’t stick on the middle of the carton lids, please do a little adjustment according the following pictures: Loosen Nut B, then use the Screw Driver to adjust the center Shaft of the tape holder. 
                     [image: ]
                                   PIC24
4、Tape  Tension  Adjustment  Shows  As The Following Picture 25:
Spin the the spinning bottom to a proper speed for the tape, then loosen Nut M8, Adjust the distance between Nut M8*50’s front and back. Change the tension of the Shaft spring to control the Tape’s tension. Spin the spinning bottom clockwise, the tape tension becomes larger, do it in the opposite direction, it becomes smaller. When you make Nut M8*50 go a little front, the tape tension becomes larger, if make it go a little back, it becomes smaller.  
[image: ]
   P.25
Tape head malfunctions and solutions


	Malfunction
	Possible reason
	Solution

	Adhesive tape can not be cut off
	The cutter is not sharp enough.
The cutter tine is jammed by the bond.
	Change the cutter
Launder and lubricate the cutter

	There is tail after the adhesive tape is cut off.

	cutter seat  is jammed ,operation is not flexible ,or the spring is not tight enough
	check all nuts on the tape head or adjust the spring tension

	The adhesive tape can’t stick to the carton completely.
	main spring is too loose to keep consistent for speed of rear wheel rebound and belt
	lock and tight the main spring nut properly

	The carton is locked in the midway.
	main spring is too tight, the front wheel is locked in midway
	loosen the main spring properly

	adhesive tape fall off easily
	one-way knurling wheel does not work
	change the knurling wheel

	carton is crooked and one carton flap is jut compared with the other after sealing
	
	the flap edge should parallel the carton body before sealing

	there is drape after sealing on tape
	
	adjust the nut M8 on the head tape to enlarge the tension as P.26

	tape alarm
	If missing tape alarm message appears first check your tape head for tape. Image. 0092
	Reset alarm as shown in image. 0093. Then reset solenoid valve as shown in image. 0094.
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P.26

4 Exploded figure

4.1 each device figure of main body as P.27,T1：                              P. 27
Part list                            T.1
	NO 
	Part No.
	Part Name
	Qty
	Remarks

	1
	GPK4001
	main machine frame
	1
	　

	
	
	
	
	

	2
	GPK4002
	store chute device
	1
	　

	
	
	
	
	

	3
	GPK4003
	[bookmark: OLE_LINK3]rear cover folding and carton pushing device
	1
	　

	
	
	
	
	

	4
	GPK4004
	carton fetching device
	1
	　

	
	
	
	
	

	5
	GPK4005
	adjusting device
	1
	　

	
	
	
	
	

	6
	GPK4006
	side cover folding device
	1
	　

	
	
	
	
	

	7
	GPK4007
	front cover folding and carton sealing device
	1
	　

	
	
	
	
	

	8
	GPK4008
	belt conveying device
	1
	　

	
	
	
	
	

	9
	GPK4009
	electric cabinet
	1
	


4.2 Main machine frame and electric cabinet figure as P.28, T2.

 P.28
Part list                                                  T.2
	NO.  
	Part No.   
	Part Name
	Qty
	Remarks

	1
	GPK40101
	connecting chute plate
	1
	　

	
	
	
	
	

	2
	GPK40102
	right standing pillar bottom sealing plate
	1
	　

	
	
	
	
	

	3
	GPK40103
	right standing pillar up sealing plate
	1
	　

	
	
	
	
	

	4
	GPK40104
	right sealing plate
	1
	　

	
	
	
	
	

	5
	GPK40105
	corner sealing plate
	1
	　

	
	
	
	
	

	6
	GPK40106
	glass guard
	1
	　

	
	
	
	
	

	7
	GPK40107
	rear sealing plate
	1
	　

	
	
	
	
	

	8
	GPK40108
	control panel
	1
	　

	
	
	
	
	

	9
	GPK40109
	electric cabinet
	1
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40110
	switch panel
	1
	

	11
	GPK40111
	electric cabinet cover
	1
	　

	
	
	
	
	

	12
	GPK40112
	left sealing plate
	1
	　

	
	
	
	
	

	13
	GPK40113
	bun foot
	4
	　

	
	
	
	
	

	14
	GPK40114
	front sealing plate
	1
	

	
	
	
	
	

	15
	
	air filter
	1
	　

	
	
	
	
	

	16
	GPK40115
	main machine frame
	1
	　

	
	
	
	
	

	17
	GPK40116
	left standing pillar bottom sealing plate
	1
	　

	
	
	
	
	

	18
	GPK40117
	rolling cover plate
	1
	　

	
	
	
	
	

	19
	GPK40118
	flowing stationary plate
	1
	　

	
	
	
	
	

	20
	GPK40119
	cover board
	1
	　

	
	
	
	
	


4.3 Store chute device figure as P.29,T3

 P. 29

Part list                             T.3                                                               
	NO  
	Part No.   
	Part Name
	Qty
	Remarks

	1
	GPK40201
	activity guide plate
	1
	　

	
	
	
	
	

	2
	GPK40202
	store chute left and right threaded rod (front) 
	1
	　

	
	
	
	
	

	3
	GPK40203
	store chute left and right tooth tube
	2
	　

	
	
	
	
	

	4
	GPK40204
	hand wheel
	1
	　

	
	
	
	
	

	5
	GPK40205
	1 chain wheel 1
	2
	　

	
	
	
	
	

	6
	GPK40206
	store chute main frame
	1
	　

	
	
	
	
	

	7
	GPK40207
	store chute left and right threaded rod(rear)
	1
	　

	
	
	
	
	

	8
	GPK40208
	standing pillar angle iron
	4
	　

	
	
	
	
	

	9
	GPK40209
	2 chain wheel 2
	2
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40210
	store chute lifting tooth tube
	2
	

	11
	GPK40211
	store chute lifting short threaded rod
	1
	　

	
	
	
	
	

	12
	GPK40212
	store chute lifting threaded rod extension shaft
	1
	　

	
	
	
	
	

	13
	GPK40213
	Store chute lifting guide shaft
	2
	　

	
	
	
	
	

	14
	GPK40214
	store chute lifting long threaded rod
	1
	

	
	
	
	
	

	15
	GPK40215
	stationary guide plate
	1
	　

	
	
	
	
	

	16
	GPK40216
	pressure plate
	1
	　

	
	
	
	
	

	17
	GPK40217
	connecting square tube
	2
	　

	
	
	
	
	

	18
	GPK40218
	U type adjusting spacer
	1
	　

	
	
	
	
	

	19
	GPK40219
	supporting bar
	1
	　

	
	
	
	
	

	20
	[bookmark: OLE_LINK1]GPK40220
	pressure guide bar
	2
	

	21
	GPK40221
	store chute slider
	1
	

	22
	GPK40222
	seat bearing
	4
	　




4.4 rear cover folding and carton pushing device figure as P.30,T4


图三十
    Part list                                T.4                                                             
	NO. 
	Part No.    
	Part Name
	Qty
	Remarks

	1
	GPK40301
	rear cover folding set piece
	1
	　

	
	
	
	
	

	2
	GPK40302
	rear cover folding shaft
	1
	　

	
	
	
	
	

	3
	GPK40303
	seat bearing
	2
	　

	
	
	
	
	

	4
	GPK40304
	rack roller carrier shaft
	1
	　

	
	
	
	
	

	5
	GPK40305
	gear
	1
	　

	
	
	
	
	

	6
	GPK40306
	rear cover folding supporting plate
	1
	　

	
	
	
	
	

	7
	GPK40307
	slider connecting plate
	1
	　

	
	
	
	
	

	8
	GPK40308
	rear cover folding supporting plate 2
	1
	　

	
	
	
	
	

	9
	GPK40309
	supporting plate
	1
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40310
	pushing bar supporting tube
	1
	

	11
	GPK40311
	pushing bar
	1
	　

	
	
	
	
	

	12
	GPK40312
	indicator
	1
	　

	
	
	
	
	

	13
	GPK40313
	radial block
	1
	　

	
	
	
	
	

	14
	GPK40314
	carton fetching slider
	1
	

	
	
	
	
	

	15
	GPK40315
	carton pushing seat
	1
	　

	
	
	
	
	

	16
	GPK40316
	adjusting silk pole
	1
	　

	
	
	
	
	

	17
	GPK40317
	prismatic locking  block
	1
	　

	
	
	
	
	

	18
	GPK40318
	carton pushing sliding shaft
	1
	　

	
	
	
	
	

	19
	PC32B200
	carton pushing cylinder
	1
	　

	
	
	
	
	

	20
	GPK40319
	guide bar shaft sleeve
	2
	

	21
	[bookmark: OLE_LINK2]GPK40220
	carton pushing cylinder seat
	1
	

	22
	GPK40221
	front cover folding cylinder seat
	2
	

	23
	PC40B30
	front cover folding cylinder
	1
	

	24
	GPK40222
	rack
	1
	　


4.5 carton fetching device figure as P.31,T.5

P.31
零件表Part list                               T.5
	NO. 
	Part No.     
	Part Name
	Qty
	Remarks

	1
	GPK40401
	（1，2）holder(1,2)
	2
	　

	
	
	
	
	

	2
	GPK40402
	auxiliary rod slider
	1
	　

	
	
	
	
	

	3
	GPK40403
	auxiliary rod
	1
	　

	
	
	
	
	

	4
	GPK40404
	auxiliary rod shaft
	1
	　

	
	
	
	
	

	5
	GPK40405
	carton fetching swinging rod connecting shaft
	1
	　

	
	
	
	
	

	6
	GPK40406
	carton fetching swinging rod
	1
	　

	
	
	
	
	

	7
	GPK40407
	nylon pad
	2
	　

	
	
	
	
	

	8
	GPK40408
	carton fetching cylinder connecting shaft
	1
	　

	
	
	
	
	

	9
	TC50B250
	carton fetching cylinder
	1
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40409
	supporting seat
	1
	

	11
	GPK40410
	carton fetching slider supporting shaft
	2
	　

	
	
	
	
	

	12
	GPK40411
	carton fetching adjusting silk shaft
	1
	　

	
	
	
	
	

	13
	GPK40412
	slider connecting plate
	1
	　

	
	
	
	
	

	14
	GPK40413
	stir shaft plate
	1
	

	
	
	
	
	

	15
	GPK40414
	prismatic locking  block
	1
	　

	
	
	
	
	

	16
	GPK40415
	buffer angle iron
	1
	　

	
	
	
	
	

	17
	GPK40416
	carton fetching slider
	2
	　

	
	
	
	
	

	18
	GPK40417
	adjusting nut plate
	1
	　

	
	
	
	
	

	19
	GPK40418
	shaft sleeve
	2
	　

	
	
	
	
	

	20
	GPK40419
	auxiliary slider shaft connecting plate
	1
	

	21
	GPK40420
	position adjustment indicator
	1
	

	22
	GPK40421
	U type spacer
	2
	

	23
	GPK40422
	suction cup
	4
	

	24
	GPK40423
	suction cup stationary plate
	2
	

	25
	GPK40424
	positioning square tube
	2
	　




4.6。adjusting device figure as P.32,T6

P.32
Part list                                       T.6
	NO.     
	Part No.             
	Part Name
	Qty  
	Remarks

	1
	GPK40501
	U type spacer
	3
	　

	
	
	
	
	

	2
	GPK40502
	positioning square tube
	3
	　

	
	
	
	
	

	3
	GPK40503
	cantilever
	1
	　

	
	
	
	
	

	4
	GPK40504
	right adjusting block
	1
	　

	
	
	
	
	

	5
	GPK40505
	middle adjusting block
	1
	　

	
	
	
	
	

	6
	GPK40506
	left adjusting block
	1
	　

	
	
	
	
	

	7
	GPK40507
	1 bearing seat 1
	2
	　

	
	
	
	
	

	8
	GPK40508
	lifting threaded rod extension shaft
	2
	　

	
	
	
	
	

	9
	GPK40509
	supporting angle iron
	1
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40510
	inner side supporting seat
	1
	



	11
	GPK40511
	Adjusting pillar
	2
	　

	
	
	
	
	

	12
	GPK40512
	Cover
	4
	　

	
	
	
	
	

	13
	GPK40513
	Lead screw
	2
	　

	
	
	
	
	

	14
	GPK40514
	Slide support shaft
	2
	

	
	
	
	
	

	15
	GPK40515
	Supporting seat 2
	2
	　

	
	
	
	
	

	16
	GPK40516
	Gear shaft
	1
	　

	
	
	
	
	

	17
	GPK40517
	Hand wheel
	1
	　

	
	
	
	
	

	18
	GPK40518
	Big gear
	1
	　

	
	
	
	
	

	19
	GPK40519
	Chain wheel
	1
	　

	
	
	
	
	

	20
	GPK40520
	Adjusting beam
	1
	

	21
	GPK40521
	Chain cover
	1
	

	22
	GPK40522
	Fixing board
	2
	

	23
	GPK40523
	Adjusting slide shaft
	4
	

	24
	GPK40524
	Top board
	1
	

	25
	GPK40525
	Side support seat
	1
	　


4.7 Side Flaps Folding Device, Image 33, Chart 7.


Image 33

Spares list                                    Chart 7
	[bookmark: _Hlk363912497]Item     
	Parts No.              
	Name
	Qty   
	Memo

	1
	GPK40601
	Driving lever
	2
	　

	
	
	
	
	

	2
	GPK40602
	Cylinder locking shaft
	2
	　

	
	
	
	
	

	3
	GPK40603
	Cylinder fixing seat
	2
	　

	
	
	
	
	

	4
	PC32B80
	Side flaps folding cylinder
	4
	　

	
	
	
	
	

	5
	GPK40604
	Joint board
	2
	　

	
	
	
	
	

	6
	GPK40605
	Bearing with seat
	4
	　

	
	
	
	
	

	7
	GPK40606
	Swing rod locating shaft
	2
	　

	
	
	
	
	

	8
	GPK40607
	Joint shaft
	2
	　

	
	
	
	
	

	9
	GPK40608
	Swing rod
	2
	　

	
	
	
	
	

	
	
	
	
	

	10
	GPK40609
	Pin type shaft
	4
	


4.8 Front flap folding and taping part, Image 34, Chart 8:

                         Image 34
Spares list                                  Chart 8
	Item     
	Parts No.              
	Name
	Qty   
	Memo

	1
	GPK40701
	Tape head
	1
	

	
	
	
	
	

	2
	GPK40702
	Joint plate 1
	2
	

	
	
	
	
	

	3
	GPK40703
	Joint plate 2
	2
	

	
	
	
	
	

	4
	GPK40704
	Support bracket
	1
	

	
	
	
	
	

	5
	GPK40705
	Cover plate
	1
	

	
	
	
	
	

	6
	GPK40706
	Cylinder seat
	4
	

	
	
	
	
	

	7
	GPK40707
	Gear rack shaft
	2
	　

	
	
	
	
	

	8
	GPK40708
	Bearing
	2
	　

	
	
	
	
	

	9
	GPK40709
	Gear rack
	2
	　

	
	
	
	
	

	10
	GPK40710
	Driving block
	1
	　

	
	
	
	
	

	11
	GPK40711
	Wheel gear
	2
	　

	
	
	
	
	

	12
	GPK40712
	Flap folding shaft
	1
	　

	
	
	
	
	

	13
	DSC320B30
	Cylinder
	2
	　

	
	
	
	
	

	
	
	
	
	


4.9 Tape Head Part, Image 35, Chart 9。

Image 35
Spares list                                   Chart 9
	Item     
	Parts No.              
	Name
	Qty   
	Memo

	1
	GPK40801
	Left plate
	1
	

	
	
	
	
	

	2
	GPK40802
	Hexagon shaft
	1
	

	
	
	
	
	

	3
	GPK40803
	Joint rod
	1
	

	
	
	
	
	

	4
	GPK40804
	Backswing
	1
	

	
	
	
	
	

	5
	GPK40805
	Knurl wheel shaft
	1
	

	
	
	
	
	

	6
	GPK40806
	Fix shaft sleeve
	2
	

	
	
	
	
	

	7
	GPK40807
	Tape support piece
	1
	　

	
	
	
	
	

	8
	GPK40808
	Guide wheel shaft
	1
	　

	
	
	
	
	

	9
	GPK40809
	PE tape guide shaft
	1
	　

	
	
	
	
	

	10
	GPK40810
	Front guide board
	1
	　

	
	
	
	
	

	11
	GPK40811
	Tape seat fix shaft
	1
	　

	
	
	
	
	

	12
	GPK40812
	Front pivot axis
	1
	　

	
	
	
	
	

	13
	GPK40813
	Knurl guide wheel
	1
	

	14
	GPK40814
	Tape wheel
	1
	

	15
	GPK40815
	PE tape guide wheel
	1
	

	16
	GPK40816
	One-way knurl wheel
	1
	

	17
	GPK40817
	Cutter soldering block
	1
	

	18
	GPK40818
	Spring locking shaft
	1
	

	19
	GPK40819
	Cutter seat fix shaft
	1
	

	20
	GPK40820
	Fix shaft sleeve
	1
	

	21
	GPK40821
	Blocking wheel
	2
	

	22
	GPK40822
	Main spring
	1
	

	23
	GPK40823
	Right plate
	1
	

	24
	GPK40824
	Plate locking shaft
	2
	

	25
	GPK40825
	Brush locking shaft
	1
	

	26
	GPK40826
	Brush 
	1
	

	27
	GPK40827
	Cutter cover
	1
	

	28
	GPK40828
	Bracket
	1
	

	29
	GPK40829
	Taping wheel
	2
	

	30
	GPK40830
	Swinging fix shaft
	2
	

	31
	GPK40831
	Taping wheel shaft
	2
	

	32
	GPK40832
	Backswing 
	1
	

	33
	GPK40833
	Tape top piece
	1
	

	34
	GPK40834
	Tape bracket
	1
	

	35
	GPK40835
	U-shape shaft sleeve
	1
	　

	
	
	
	
	

	
	
	
	
	


4.10 Belts conveying device, Image 36, Chart 10:

Image 36
Spares list                                 Chart 8
	Item     
	Parts No.              
	Name
	Qty   
	Memo

	1
	GPK40901
	Belt cover
	2
	

	
	
	
	
	

	2
	GPK40902
	Conveying belt
	2
	

	
	
	
	
	

	3
	GPK40903
	Drive wheel
	2
	

	
	
	
	
	

	4
	GPK40904
	Drive wheel shaft
	2
	

	
	
	
	
	

	5
	GPK40905
	Belt cover support rod
	4
	

	
	
	
	
	

	6
	GPK40906
	Driven wheel
	2
	

	
	
	
	
	

	7
	GPK40907
	Driven wheel shaft
	2
	　

	
	
	
	
	

	8
	GPK40908
	belt guide plate
	2
	　

	
	
	
	
	

	9
	GPK40909
	Belt cover support
	2
	　

	
	
	
	
	

	10
	GPK40910
	Belt support seat
	4
	　

	
	
	
	
	

	11
	GPK40911
	Support barrel
	4
	　

	
	
	
	
	

	12
	GPK40912
	Driven lead screw
	1
	　

	
	
	
	
	

	13
14

	GPK40913
	Chain wheel
	2
	

	14
15
	GPK40914
	Drive lead screw
	1
	

	15
	GPK40915
	Motor
	2
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